**OBJECTIVE**

* To carry out an assessment to determine if there is any risk that may contaminate the mangos or the growing areas.

**PREVENTIVE MEASURES**

* Before starting work, an inspection of the equipment to be used during the day is performed.
* The equipment is inspected to verify that it is clean and in good working condition.
* All areas of potential sources of physical and chemical hazards are inspected such as:
* Drip trays are in place and firmly secured.
* Chemicals, oils, fats and combustibles should be kept out of the crop field.
* The hydraulic hoses, motors and fittings must be tight; they should not leak and must not have any signs of leaks or drips.
* The pieces of equipment that are loose or damaged are removed or repaired immediately.
* Any foreign material (glass, metal, wood, etc.) embedded in the pieces of the harvesting equipment should be removed.
* The evaluation is documented and corrective actions are entered in the document (REG-PREHARV3.1.2).