**OBJECTIVE**

* + To ensure the cleanliness of the mangos to remove the dust and resin that is naturally found in this product so it does not become a source of contamination.

**GENERAL PROCEDURE**

* The water used to wash the mangos is suitable for this use (REG-CTRLWAPP-5.2.2).
* The water used for washing the mangos is treated with a disinfectant as indicated in the procedure for the Control and Management of Microbial Agents in the Water (POE-ANTIMICAG-5.2.6)
* The concentration of antimicrobial agents is recorded, using the Register of Monitoring of the Concentration of Disinfectant in the Water (REG-MCDAW-5.2.7).

**WASHING PROCEDURES IN AN IMMERSION TUB**

* The mangos are submerged in a tub of water and advance through a current produced inside the tub to a series of rollers, boards, or strips that remove them from the tub to then pass to the selection stage.

**WASHING PROCEDURES BY SPRAYING**

* The mangos are transported through a series of rollers where they are sprayed with a solution of water with disinfectant and then passed to the selection stage.